Host CTO_LtJG_Telarus says:
CEO: Hello
Host CTO_LtJG_Telarus says:
Yates: Lt. always a pleasure.
Lieutenant_Ashley_Yates says:
::Steps in::
Lieutenant_Ashley_Yates says:
Telarus: Hello again Lieutenant. ::Smiles::
Host CTO_LtJG_Telarus says:
All: Well let's get started.
CEO_ENS_Ivanova says:
Yates: Pleasure meeting you again.
Lieutenant_Ashley_Yates says:
Sure. ::smiles::
Host CTO_LtJG_Telarus says:
Computer: Activate Display...show us a standard Warp Core Design for an Excelsior Class Vessel show the USS Excelsior's NX-2000 Original Warp X Design and it's control system.
Host CTO_LtJG_Telarus says:
All: You will all see here that the Original NX-2000 Excelsior had a Warp X core. It was removed and replaced with a more reliable after Captain Scott sabotaged it and was able to undermine the system that controlled the Warp X system by only removing a few isolinear chips.
CEO_ENS_Ivanova says:
::whispers self:: That wasn't the only reason it failed.
Host CTO_LtJG_Telarus says:
All: Excuse me Ensign what comment do you have to share, please I invite all criticisms ideas and so forth.
CEO_ENS_Ivanova says:
Telarus: Sir part of the problem with the original Trans Warp experiment were the power requirements were higher then could be down at the time
Host CTO_LtJG_Telarus says:
CEO: With recent advancements in design to our current power systems, we have enough now I believe I also have recalculated the SIF calculations to adjust for the extreme stress on the hull plating.
CEO_ENS_Ivanova says:
CEO: Alright let’s see if it works.
Cdt_John says:
Ok.
Host CTO_LtJG_Telarus says:
All: I have already run tests on shuttles with another CEO, Chief K'Vas of the USS Delphyne and I had a conference today with him in his seminar and we brought up my Warp X project and we raced to shuttles one with the Warp X drive and another with a regular set up.
Host CTO_LtJG_Telarus says:
All: It passed the stress tests and fuel consumption has been reduced dramatically to only 10% over the current fuel consumption standard.
Cdt_John says:
Ah.
CEO_ENS_Ivanova says:
Only 10 percent
Cdt_John says:
Pretty good
CEO_ENS_Ivanova says:
Still it is only shuttles
Cdt_John says:
Pretty good, although shouldn’t there be some test on freighters, or something a little larger?
Host CTO_LtJG_Telarus says:
All: I had to use shuttles for the time being, I should make a correction I have found here on the LCARS network. It was actually duotronic control chips; this would even further worsen the case against the old control system created by Dr.  Tokogawa and the NNEC
Host CTO_LtJG_Telarus says:
All: We now use bio-neural gel packs and isolinear control chips. With my new system I use the gel packs which are better processors and have better safeguards and fail safes.
CEO_ENS_Ivanova says:
What about preventing infection from bacteria sir.
Host CTO_LtJG_Telarus says:
CEO: That is why we will have weekly check ups by Medical on the system, but just incase we have an isolinear chip back up that is just as efficient.
Host CTO_LtJG_Telarus says:
CEO: All the packs are inoculated with the latest anti-viral agents.
CEO_ENS_Ivanova says:
CEO: What about nanobot’ infections?
Host CTO_LtJG_Telarus says:
CEO: This control system would be magnetically sealed and would have also no external connections other than what is necessary, the magnetic field surrounding the chamber housing the control system prevents nanobots from entering because the magnetic seal creates a field that it would fry any nanobot.